**OLLINS LANDE SOLO TECHNICAL REQUIREMENTS (June 2017)**

1. If Backline provided: 1 vocal mics with stand and XLR lead

1 instrument mic (for cajon) with low stand and XLR lead if required

1 DI inputs for guitar plus instrument jack leads

1 standard AC power socket available (for lead guitar pedal board)

2. If no Backline provided: 2 standard AC power sockets

Ideally at least 8 feet x 5 feet floor space and location for PAs

For option 1 above, Ollins can supply all mics, stands and leads if none provided with backline. We can also input straight into sound desk if no DI boxes available.